**ICAM5 - 2019**

**TOPIC:**CORROSION / WELDING

**TITLE:**UNDERSTANDING SULFIDE STRESS CRACKING RESISTANCE OF BUTT WELDS WITH MICROSCOPIC DEFECTS

**AUTHOR:**

ALAGARASAN GOVINDHAN, SAPURAENERGY, ALAGARASAN.G@SAPURAENERGY.COM, +60 19 245 4916

VARUN PRAKASH, SAPURAENERGY,   
VARUN.PRAKASH@SAPURAENERGY.COM, +60 17 3410 881

SHASHI BHUSHAN KUMAR, DNVGL,  
SHASHI.BHUSHAN.KUMAR@DNVGL.COM, +65 9711 2996

**KEYWORDS**

CORROSION, WELDING, GIRTH WELDS, BUTT WELDS, SSC

**ABSTRACT**

In recent years, offshore explorations in the Oil & Gas industry have resulted in harsher well fluids containing significant hydrogen sulﬁde (H2S). Transportation of such fluid from remote offshore location to land are by long pipelines produced by butt welding in circumferential direction. These circumferential butt welds are also known as girth welds. One common failure mode for such pipelines are cracking under the combined action of H2S, tensile stress and water. This requires girth welds with improved cracking resistance in aggressive hydrogen sulﬁde-containing medium, termed as sour service. This paper intends to discuss the corrosion resistance requirements of girth welds with particular focus on sulfide stress cracking. A case study addressing the typical welding processes, types of corrosion tests, specimen preparation, non-destructive testing requirements, testing procedure and evaluations will be presented. The different test conditions recommended will be discussed. Final evaluation criteria of international standards will also be presented. The interpretations of microscopic defects as welding procedure failure will also be discussed. Finally, best practise for laboratory examination and due diligence initiatives on specimen validity will be suggested.